Filetype: IR signals file
Version: 1
#
name: KEY_SETUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: band
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: SPEEDright
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: goto
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: rep
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: KEY_TITLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: KEY_ANGLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: sel
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 40 00 00 00
#
name: L/R
type: parsed
protocol: NECext
address: 00 00 00 00
command: 48 00 00 00
#
name: root
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4C 00 00 00
#
name: KEY_0+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4D 00 00 00
#
name: SPEEDleft
type: parsed
protocol: NECext
address: 00 00 00 00
command: 54 00 00 00
