Filetype: IR signals file
Version: 1
#
name: KEY_BACK
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 00 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 01 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 02 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 03 00 00 00
#
name: KEY_EXIT
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 04 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 05 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 06 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 07 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 08 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 09 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0A 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0B 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0C 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0D 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0E 00 00 00
#
name: KEY_EPG
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 0F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 10 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 11 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 12 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 14 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 15 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 16 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 18 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 19 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 1A 00 00 00
#
name: KEY_CLEAR
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 1C 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 1D 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 1E 00 00 00
#
name: KEY_MODE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 50 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 51 00 00 00
#
name: AB
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 52 00 00 00
#
name: KEY_AUDIO
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 53 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 54 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 55 00 00 00
#
name: KEY_TITLE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 56 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 57 00 00 00
#
name: KEY_ZOOM
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 58 00 00 00
#
name: KEY_ANGLE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 59 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5A 00 00 00
#
name: SoundMode
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5B 00 00 00
#
name: KEY_EJECTCD
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5C 00 00 00
#
name: TVSystem
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5D 00 00 00
#
name: Goto
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5E 00 00 00
#
name: KEY_SLOW
type: parsed
protocol: NECext
address: 80 6E 00 00
command: 5F 00 00 00
