Filetype: IR signals file
Version: 1
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 07 00 00 00
command: 01 00 00 00
#
name: CTVERECVECTVERCI
type: parsed
protocol: NECext
address: 07 00 00 00
command: 02 00 00 00
#
name: A_RED
type: parsed
protocol: NECext
address: 07 00 00 00
command: 03 00 00 00
#
name: B_GREEN
type: parsed
protocol: NECext
address: 07 00 00 00
command: 04 00 00 00
#
name: C_YELLOW
type: parsed
protocol: NECext
address: 07 00 00 00
command: 05 00 00 00
#
name: OTAZNIK_BLUE
type: parsed
protocol: NECext
address: 07 00 00 00
command: 06 00 00 00
#
name: CH_PLUS
type: parsed
protocol: NECext
address: 07 00 00 00
command: 08 00 00 00
#
name: CH_MINUS
type: parsed
protocol: NECext
address: 07 00 00 00
command: 09 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0A 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0B 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0C 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0D 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0E 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 07 00 00 00
command: 0F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 07 00 00 00
command: 11 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 07 00 00 00
command: 12 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 07 00 00 00
command: 14 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 07 00 00 00
command: 15 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 07 00 00 00
command: 17 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 07 00 00 00
command: 18 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 07 00 00 00
command: 1A 00 00 00
#
name: CAPS_NUM
type: parsed
protocol: NECext
address: 07 00 00 00
command: 1B 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 07 00 00 00
command: 1D 00 00 00
#
name: DEL
type: parsed
protocol: NECext
address: 07 00 00 00
command: 1E 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 07 00 00 00
command: 20 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 07 00 00 00
command: 21 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: 07 00 00 00
command: 22 00 00 00
#
name: BEGINNING
type: parsed
protocol: NECext
address: 07 00 00 00
command: 23 00 00 00
#
name: KEY_END
type: parsed
protocol: NECext
address: 07 00 00 00
command: 24 00 00 00
#
name: CTVERECSETREMIRADKY
type: parsed
protocol: NECext
address: 07 00 00 00
command: 25 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 07 00 00 00
command: 26 00 00 00
#
name: KEY_EPG
type: parsed
protocol: NECext
address: 07 00 00 00
command: 27 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 07 00 00 00
command: 28 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 07 00 00 00
command: 29 00 00 00
#
name: JUMP
type: parsed
protocol: NECext
address: 07 00 00 00
command: 2A 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 07 00 00 00
command: 2B 00 00 00
#
name: KEY_BACK
type: parsed
protocol: NECext
address: 07 00 00 00
command: 30 00 00 00
#
name: PINNACLE
type: parsed
protocol: NECext
address: 07 00 00 00
command: 33 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 07 00 00 00
command: 36 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 07 00 00 00
command: 39 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 07 00 00 00
command: 3C 00 00 00
#
name: RED_IN_THE_MIDDLE
type: parsed
protocol: NECext
address: 07 00 00 00
command: 3F 00 00 00
