Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 09 00 00 00
#
name: ch+
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 0D 00 00 00
#
name: ch-
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 0E 00 00 00
#
name: previous
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 0F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 11 00 00 00
#
name: menu
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 20 00 00 00
#
name: up
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 21 00 00 00
#
name: down
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 22 00 00 00
#
name: left
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 23 00 00 00
#
name: right
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 24 00 00 00
#
name: enter
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 25 00 00 00
#
name: exit
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 26 00 00 00
#
name: back
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 27 00 00 00
#
name: guide
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 28 00 00 00
#
name: info
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 2E 00 00 00
#
name: play
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 30 00 00 00
#
name: stop
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 31 00 00 00
#
name: pause
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 32 00 00 00
#
name: skip-
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 33 00 00 00
#
name: skip+
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 34 00 00 00
#
name: record
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 35 00 00 00
#
name: red
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 41 00 00 00
#
name: yellow
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 42 00 00 00
#
name: green
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 43 00 00 00
#
name: blue
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 44 00 00 00
#
name: vol+
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 59 00 00 00
#
name: vol-
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 59 00 00 00
#
name: mute
type: parsed
protocol: NECext
address: 0C 00 00 00
command: 59 00 00 00
