Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 09 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0A 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0B 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0C 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 11 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 12 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 13 00 00 00
#
name: KEY_CYCLEWINDOWS
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 1E 00 00 00
#
name: KEY_TEXT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 21 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 25 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 26 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 27 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 28 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 29 00 00 00
#
name: pre-ch
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2A 00 00 00
#
name: pip
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2B 00 00 00
#
name: KEY_SLEEP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2C 00 00 00
#
name: KEY_VIDEO
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 30 00 00 00
#
name: scart
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 31 00 00 00
#
name: KEY_PC
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 32 00 00 00
#
name: dtvmenu
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 33 00 00 00
#
name: KEY_ZOOMOUT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 34 00 00 00
#
name: mix
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 35 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 36 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 37 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 40 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 45 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 46 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 47 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 49 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 70 00 00 00
#
name: KEY_EXIT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 71 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 72 00 00 00
#
name: index
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 73 00 00 00
#
name: sound
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 74 00 00 00
#
name: KEY_ZOOMIN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 79 00 00 00
#
name: size
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 86 00 00 00
#
name: reveal
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 87 00 00 00
#
name: hold
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 88 00 00 00
