Filetype: IR signals file
Version: 1
# 
# ElecHome SH8820 Humidifier
# 
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
# 
name: MinMax
type: parsed
protocol: NEC
address: 00 00 00 00
command: 03 00 00 00
# 
name: ChildLock
type: parsed
protocol: NEC
address: 00 00 00 00
command: 57 00 00 00
# 
name: HumiLevel
type: parsed
protocol: NEC
address: 00 00 00 00
command: 17 00 00 00
