Filetype: IR signals file
Version: 1
#
name: KEY_STOP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 00 00 00 00
#
name: KEY_OPEN
type: parsed
protocol: NECext
address: B0 00 00 00
command: 01 00 00 00
#
name: Rev
type: parsed
protocol: NECext
address: B0 00 00 00
command: 04 00 00 00
#
name: KEY_FORWARD
type: parsed
protocol: NECext
address: B0 00 00 00
command: 05 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 06 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 0A 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: B0 00 00 00
command: 10 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: B0 00 00 00
command: 11 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: B0 00 00 00
command: 12 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: B0 00 00 00
command: 13 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: B0 00 00 00
command: 14 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: B0 00 00 00
command: 15 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: B0 00 00 00
command: 16 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: B0 00 00 00
command: 17 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: B0 00 00 00
command: 18 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: B0 00 00 00
command: 19 00 00 00
#
name: KEY_AUDIO
type: parsed
protocol: NECext
address: B0 00 00 00
command: 33 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: B0 00 00 00
command: 3D 00 00 00
#
name: A-B_Repeat
type: parsed
protocol: NECext
address: B0 00 00 00
command: 48 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: B0 00 00 00
command: 49 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: B0 00 00 00
command: 4A 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: B0 00 00 00
command: 80 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: B0 00 00 00
command: 81 00 00 00
#
name: KEY_SELECT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 82 00 00 00
#
name: KEY_CLEAR
type: parsed
protocol: NECext
address: B0 00 00 00
command: 83 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 85 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: B0 00 00 00
command: 86 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 87 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: B0 00 00 00
command: 88 00 00 00
#
name: >=10
type: parsed
protocol: NECext
address: B0 00 00 00
command: 89 00 00 00
#
name: RepeatMode
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8C 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8D 00 00 00
#
name: Marker
type: parsed
protocol: NECext
address: B0 00 00 00
command: 8E 00 00 00
#
name: KEY_ANGLE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 90 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 91 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: B0 00 00 00
command: 92 00 00 00
#
name: KEY_SETUP
type: parsed
protocol: NECext
address: B0 00 00 00
command: 94 00 00 00
#
name: KEY_TITLE
type: parsed
protocol: NECext
address: B0 00 00 00
command: 9B 00 00 00
#
name: VSS
type: parsed
protocol: NECext
address: B0 00 00 00
command: 9E 00 00 00
