Filetype: IR signals file
Version: 1
#
name: MUTE
type: parsed
protocol: NECext
address: BA A0 00 00
command: 01 00 00 00
#
name: VOLUME_-
type: parsed
protocol: NECext
address: BA A0 00 00
command: 02 00 00 00
#
name: VOLUME_+
type: parsed
protocol: NECext
address: BA A0 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: BA A0 00 00
command: 4C 00 00 00
