Filetype: IR signals file
Version: 1
#
name: KEY_1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_10CHANNELSUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_MODE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_TAB
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_ZOOM
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK--
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK++
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_EJECTCD
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_10CHANNELSUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_MODE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_TAB
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_ZOOM
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK--
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK++
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_EJECTCD
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_F4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
