Filetype: IR signals file
Version: 1
# 
name: Volume_up
type: parsed
protocol: NECext
address: BA A0 00 00
command: 03 FC 00 00
# 
name: Volume_down
type: parsed
protocol: NECext
address: BA A0 00 00
command: 02 FD 00 00
# 
name: Mode_aux
type: parsed
protocol: NECext
address: BA A0 00 00
command: 0D F2 00 00
# 
name: Mode_bt
type: parsed
protocol: NECext
address: BA A0 00 00
command: 81 7E 00 00
# 
name: Power
type: parsed
protocol: NECext
address: BA A0 00 00
command: 4C B3 00 00