Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 80 37 00 00
command: 20 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: 80 37 00 00
command: 21 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 80 37 00 00
command: 22 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 80 37 00 00
command: 23 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 80 37 00 00
command: 25 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: 80 37 00 00
command: 26 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: 80 37 00 00
command: 27 00 00 00
#
name: CHAPTER_<<
type: parsed
protocol: NECext
address: 80 37 00 00
command: 28 00 00 00
#
name: CHAPTER_>>
type: parsed
protocol: NECext
address: 80 37 00 00
command: 29 00 00 00
#
name: GOUP_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 2A 00 00 00
#
name: GROUP_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 2B 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 80 37 00 00
command: 30 00 00 00
#
name: BROADCAST
type: parsed
protocol: NECext
address: 80 37 00 00
command: 31 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 80 37 00 00
command: 32 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 33 00 00 00
#
name: FUNCTION_3
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3D 00 00 00
#
name: RECEIVER_MUTE
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3D 00 00 00
#
name: FUNCTION_1
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3E 00 00 00
#
name: RECEIVER_VOL_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3E 00 00 00
#
name: FUNCTION_2
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3F 00 00 00
#
name: RECEIVER_VOL_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 3F 00 00 00
#
name: ARTIST
type: parsed
protocol: NECext
address: 80 37 00 00
command: 40 00 00 00
#
name: ALBUM
type: parsed
protocol: NECext
address: 80 37 00 00
command: 41 00 00 00
#
name: GENRES
type: parsed
protocol: NECext
address: 80 37 00 00
command: 42 00 00 00
#
name: ALL_SONGS
type: parsed
protocol: NECext
address: 80 37 00 00
command: 43 00 00 00
#
name: PLAYLIST
type: parsed
protocol: NECext
address: 80 37 00 00
command: 44 00 00 00
#
name: SONG_STATS.
type: parsed
protocol: NECext
address: 80 37 00 00
command: 45 00 00 00
#
name: BOOKMARKS
type: parsed
protocol: NECext
address: 80 37 00 00
command: 46 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 80 37 00 00
command: 47 00 00 00
#
name: RECORDING
type: parsed
protocol: NECext
address: 80 37 00 00
command: 48 00 00 00
#
name: AV_RECIEVER
type: parsed
protocol: NECext
address: 80 37 00 00
command: 49 00 00 00
#
name: CLIENT_PLAYBACK
type: parsed
protocol: NECext
address: 80 37 00 00
command: 4A 00 00 00
#
name: EXT._INPUTS
type: parsed
protocol: NECext
address: 80 37 00 00
command: 4B 00 00 00
#
name: PLAY_INFO
type: parsed
protocol: NECext
address: 80 37 00 00
command: 4E 00 00 00
#
name: BOOKMARK_ON/OFF
type: parsed
protocol: NECext
address: 80 37 00 00
command: 4F 00 00 00
#
name: TOP_MENU
type: parsed
protocol: NECext
address: 80 37 00 00
command: 50 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 80 37 00 00
command: 51 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 80 37 00 00
command: 52 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 80 37 00 00
command: 53 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 54 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 55 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 56 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 80 37 00 00
command: 57 00 00 00
#
name: SUB_MENU
type: parsed
protocol: NECext
address: 80 37 00 00
command: 58 00 00 00
#
name: PAGE_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 59 00 00 00
#
name: PAGE_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 5A 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 80 37 00 00
command: 61 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 80 37 00 00
command: 80 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 80 37 00 00
command: 82 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 80 37 00 00
command: 83 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 80 37 00 00
command: 83 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 80 37 00 00
command: 85 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 80 37 00 00
command: 85 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 80 37 00 00
command: 86 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: 80 37 00 00
command: 86 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 80 37 00 00
command: 87 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: 80 37 00 00
command: 87 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 80 37 00 00
command: 88 00 00 00
#
name: CHAPTER_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 88 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 80 37 00 00
command: 89 00 00 00
#
name: CHAPTER_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 89 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8A 00 00 00
#
name: GROUP_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8A 00 00 00
#
name: GROUP_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8B 00 00 00
#
name: FAVORITE_1
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8C 00 00 00
#
name: FAVORITE_2
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8D 00 00 00
#
name: FAVORITE_3
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8E 00 00 00
#
name: FAVORITE_4
type: parsed
protocol: NECext
address: 80 37 00 00
command: 8F 00 00 00
#
name: BOOKMARK
type: parsed
protocol: NECext
address: 80 37 00 00
command: 91 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 80 37 00 00
command: 92 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 93 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 80 37 00 00
command: 98 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 80 37 00 00
command: 9D 00 00 00
#
name: VOLUME_-
type: parsed
protocol: NECext
address: 80 37 00 00
command: 9E 00 00 00
#
name: VOLUME_+
type: parsed
protocol: NECext
address: 80 37 00 00
command: 9F 00 00 00
#
name: PLAY_INFO
type: parsed
protocol: NECext
address: 80 37 00 00
command: AE 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 80 37 00 00
command: B1 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 80 37 00 00
command: B2 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 80 37 00 00
command: B3 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 80 37 00 00
command: B4 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 80 37 00 00
command: B5 00 00 00
#
name: SELECT/ENTER
type: parsed
protocol: NECext
address: 80 37 00 00
command: B6 00 00 00
#
name: LIBRARY
type: parsed
protocol: NECext
address: 80 37 00 00
command: BD 00 00 00
#
name: OFF_TIMER
type: parsed
protocol: NECext
address: 80 37 00 00
command: BE 00 00 00
#
name: ON_TIMER
type: parsed
protocol: NECext
address: 80 37 00 00
command: BF 00 00 00
