Filetype: IR signals file
Version: 1
#
name: audiodown
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 00 00 00 00
#
name: int/ext
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 01 00 00 00
#
name: dec
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 02 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 03 00 00 00
#
name: mo/st
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 06 00 00 00
#
name: audioup
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 07 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 09 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 0A 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 0D 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 0E 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 0F 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 10 00 00 00
#
name: KEY_VIDEO
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 11 00 00 00
#
name: KEY_VIDEO
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 12 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 15 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 16 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 17 00 00 00
#
name: h/v
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 19 00 00 00
#
name: dev
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1A 00 00 00
#
name: p-aud
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1B 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1C 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1D 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1E 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 8A F5 00 00
command: 1F 00 00 00
