Filetype: IR signals file
Version: 1
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 00 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 01 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 02 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 03 00 00 00
#
name: PROG
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 04 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 05 00 00 00
#
name: ADD/DEL
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 06 00 00 00
#
name: AUTO
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 07 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 08 00 00 00
#
name: MUTE/RESET
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 09 00 00 00
#
name: PICTURE
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 0B 00 00 00
#
name: KEY_VIDEO
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 0C 00 00 00
#
name: SAP
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 0D 00 00 00
#
name: KEY_SLEEP
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 0E 00 00 00
#
name: X_KEY_0/AM/PM
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 10 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 11 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 12 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 13 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 14 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 15 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 16 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 17 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 18 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 19 00 00 00
#
name: Q.REV
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 1A 00 00 00
#
name: KEY_AGAIN
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 1B 00 00 00
#
name: CLK/TIM
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 1C 00 00 00
#
name: SET
type: parsed
protocol: NECext
address: 83 7A 00 00
command: 1F 00 00 00
