Filetype: IR signals file
Version: 1
#
name: TV/VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0F 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 10 00 00 00
#
name: VOLUME_+
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1A 00 00 00
#
name: VOLUME_-
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1E 00 00 00
