Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: TXT-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: PP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: b6_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 22 00 00 00
#
name: b7_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: b8_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 24 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: HOLD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: KEY_TIME
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: b10_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: ?
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: KEY_X
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: MIX
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: Psz
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: b11_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: Pst
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: Pon
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: SEL
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3B 00 00 00
#
name: KEY_TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
