Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 09 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0A 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0B 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0D 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0E 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 11 00 00 00
#
name: KEY_AGAIN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 12 00 00 00
#
name: UpArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 14 00 00 00
#
name: DownArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 15 00 00 00
#
name: LeftArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 16 00 00 00
#
name: RightArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 17 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1B 00 00 00
#
name: SkipForward
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1E 00 00 00
#
name: KEY_EXIT
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1F 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 20 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 21 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 24 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 25 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 29 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 2E 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 30 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 32 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 34 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 35 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 36 00 00 00
#
name: KEY_RECORD
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 37 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 38 00 00 00
