Filetype: IR signals file
Version: 1
#
name: KEY_1
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 00 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 01 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 02 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 03 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 04 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 05 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 06 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 07 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 08 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 09 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 0B 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 0B 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 10 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 11 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 15 00 00 00
#
name: KEY_EJECTCD
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 16 00 00 00
#
name: KEY_AUDIO
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 17 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 18 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 19 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 1A 00 00 00
#
name: KEY_BACK
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 1B 00 00 00
#
name: KEY_FORWARD
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 1C 00 00 00
#
name: KEY_RECORD
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 1D 00 00 00
#
name: surround
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 1E 00 00 00
#
name: top-menu
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 22 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 23 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 24 00 00 00
#
name: tv/video
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 2A 00 00 00
#
name: bookmark/search-menu
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 30 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 42 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 43 00 00 00
#
name: KEY_SETUP
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 4D 00 00 00
#
name: input-select
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 4F 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 56 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 57 00 00 00
#
name: sp/ep
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 58 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 5A 00 00 00
#
name: repeat/replay
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 5B 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 5D 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 60 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 61 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 62 00 00 00
#
name: KEY_CLEAR
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 63 00 00 00
#
name: KEY_ANGLE
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 65 00 00 00
#
name: select-video
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 69 00 00 00
#
name: select-dvd
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 6A 00 00 00
#
name: muting/zoom
type: parsed
protocol: NECext
address: 1A 53 00 00
command: 79 00 00 00
