Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 09 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0A 00 00 00
#
name: vt
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0B 00 00 00
#
name: av
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0C 00 00 00
#
name: X_KEY_0+
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0D 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0E 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 0F 00 00 00
#
name: picture
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 10 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 11 00 00 00
#
name: exp
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 13 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 14 00 00 00
#
name: timer
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 15 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 16 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 17 00 00 00
#
name: hold
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 18 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 19 00 00 00
#
name: mix
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1A 00 00 00
#
name: reveal
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1B 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1C 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1D 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1E 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 0B 0B 00 00
command: 1F 00 00 00
