Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 09 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 10 00 00 00
#
name: T-Shift
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 11 00 00 00
#
name: HiFi
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 12 00 00 00
#
name: Mts/Srs
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 13 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 14 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 16 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 17 00 00 00
#
name: KEY_FORWARD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 18 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1A 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1B 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1E 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1F 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 40 00 00 00
#
name: Fm/Am
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 41 00 00 00
#
name: KEY_MP3
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 42 00 00 00
#
name: KEY_IMAGES
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 43 00 00 00
#
name: KEY_VIDEO
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 44 00 00 00
#
name: KEY_DVD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 45 00 00 00
#
name: KaraOk
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 46 00 00 00
#
name: Ap
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 47 00 00 00
#
name: KEY_RECORD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 48 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 49 00 00 00
#
name: KEY_EXIT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 4E 00 00 00
#
name: Ttx
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 4F 00 00 00
#
name: KEY_HOME
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 52 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 53 00 00 00
#
name: KEY_AGAIN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 55 00 00 00
#
name: Set
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 57 00 00 00
#
name: Eq
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 58 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 59 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5A 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5B 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5C 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5D 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5E 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 5F 00 00 00
