Filetype: IR signals file
Version: 1
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 80 26 00 00
command: 01 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 80 26 00 00
command: 02 00 00 00
#
name: KEY_KPMINUS
type: parsed
protocol: NECext
address: 80 26 00 00
command: 07 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 80 26 00 00
command: 08 00 00 00
#
name: V/H
type: parsed
protocol: NECext
address: 80 26 00 00
command: 0A 00 00 00
#
name: MEM
type: parsed
protocol: NECext
address: 80 26 00 00
command: 0B 00 00 00
#
name: KEY_KPPLUS
type: parsed
protocol: NECext
address: 80 26 00 00
command: 0C 00 00 00
#
name: SET
type: parsed
protocol: NECext
address: 80 26 00 00
command: 0D 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 80 26 00 00
command: 0F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 80 26 00 00
command: 11 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 80 26 00 00
command: 12 00 00 00
#
name: KEY_AUDIO
type: parsed
protocol: NECext
address: 80 26 00 00
command: 14 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 80 26 00 00
command: 15 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 80 26 00 00
command: 16 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 80 26 00 00
command: 17 00 00 00
#
name: P/L
type: parsed
protocol: NECext
address: 80 26 00 00
command: 18 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 80 26 00 00
command: 19 00 00 00
#
name: D/ON
type: parsed
protocol: NECext
address: 80 26 00 00
command: 1A 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 80 26 00 00
command: 1B 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 80 26 00 00
command: 1D 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 80 26 00 00
command: 1E 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 80 26 00 00
command: 1F 00 00 00
