Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: KEY_1-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: KEY_2-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: tv_off
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: vcr_off
type: parsed
protocol: NECext
address: 06 00 00 00
command: 0C 00 00 00
#
name: toggle_sound
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: reverse_corner
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: uhr_corner
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: fa
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: uhr_music
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: quiz
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: program+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: program-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: contrast+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: ra_sl_us
type: parsed
protocol: NECext
address: 00 00 00 00
command: 28 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 06 00 00 00
command: 29 00 00 00
#
name: color-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: brightness-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: brightness+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: color+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: contrast-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2F 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 06 00 00 00
command: 32 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: 06 00 00 00
command: 34 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 06 00 00 00
command: 35 00 00 00
#
name: corner
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 06 00 00 00
command: 36 00 00 00
#
name: KEY_M
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: KEY_RECORD
type: parsed
protocol: NECext
address: 06 00 00 00
command: 37 00 00 00
#
name: av
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: s100
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3A 00 00 00
#
name: KEY_TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3E 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
