Filetype: IR signals file
Version: 1
# 
# Samsung H6300 TV
#
name: Power
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: Source
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: 1
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 04 00 00 00
# 
name: 2
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 05 00 00 00
# 
name: 3
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 06 00 00 00
# 
name: 4
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 08 00 00 00
# 
name: 5
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 09 00 00 00
# 
name: 6
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0A 00 00 00
# 
name: 7
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0C 00 00 00
# 
name: 8
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0D 00 00 00
# 
name: 9
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0E 00 00 00
# 
name: 0
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 11 00 00 00
# 
name: TTX_MIX
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2C 00 00 00
# 
name: PRE_CH
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 13 00 00 00
# 
name: Vol_Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: Vol_Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: Mute
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: CH_Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: CH_Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
# 
name: CH_List
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: Menu
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: Guide
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: Tools
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4B 00 00 00
# 
name: Info
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1F 00 00 00
# 
name: Smart_Hub
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 79 00 00 00
# 
name: UP
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: DOWN
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: LEFT
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: RIGHT
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: Enter
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Return
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: A
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6C 00 00 00
# 
name: B
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 14 00 00 00
# 
name: C
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 15 00 00 00
# 
name: D
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 16 00 00 00
# 
name: Soccer_Mode
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: B8 00 00 00
# 
name: Search
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 73 00 00 00
# 
name: Keypad
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: D2 00 00 00
# 
name: E_Manual
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3F 00 00 00
# 
name: P_Size
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3E 00 00 00
# 
name: AD_Subt
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 25 00 00 00
# 
name: Backwards
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 45 00 00 00
# 
name: Pause
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4A 00 00 00
# 
name: Play
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 47 00 00 00
# 
name: Forwards
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 48 00 00 00
# 
name: Record
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 49 00 00 00
# 
name: Stop
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 46 00 00 00
