Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 01 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 01 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 01 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 01 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 01 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 01 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 01 00 00 00
command: 09 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0F 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 01 00 00 00
command: 14 00 00 00
#
name: ARROW_UP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 16 00 00 00
#
name: ARROW_LEFT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 17 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 19 00 00 00
#
name: ARROW_DOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1D 00 00 00
#
name: TV/SAT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1E 00 00 00
#
name: TV/RADIO
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1F 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 01 00 00 00
command: 24 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 25 00 00 00
#
name: STREAM
type: parsed
protocol: NECext
address: 01 00 00 00
command: 28 00 00 00
#
name: KEY_ESC
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2D 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 31 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 33 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 35 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 38 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 3A 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 3C 00 00 00
