Filetype: IR signals file
Version: 1
#
name: KEY_OPEN
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 00 00 00 00
#
name: RightArrow
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 01 00 00 00
#
name: UpArrow
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 02 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 03 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 04 00 00 00
#
name: DownArrow
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 05 00 00 00
#
name: LeftArrow
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 06 00 00 00
#
name: KEY_ENTER
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 07 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 08 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 09 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0A 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0B 00 00 00
#
name: KEY_FORWARD
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0C 00 00 00
#
name: Rev
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0D 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0E 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 0F 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 10 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 11 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 12 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 14 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 15 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 16 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 18 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 19 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 1A 00 00 00
#
name: Network
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 1C 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 1D 00 00 00
#
name: KEY_CLEAR
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 1E 00 00 00
#
name: KEY_SLOW
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 50 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 51 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 52 00 00 00
#
name: KEY_TITLE
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 53 00 00 00
#
name: KEY_AUDIO
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 54 00 00 00
#
name: KEY_SUBTITLE
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 55 00 00 00
#
name: KEY_ANGLE
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 56 00 00 00
#
name: Zoom/View
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 57 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 58 00 00 00
#
name: PS/IS
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 59 00 00 00
#
name: KEY_SEARCH
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5A 00 00 00
#
name: Enhance
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5B 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5C 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5D 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5E 00 00 00
#
name: KEY_SETUP
type: parsed
protocol: NECext
address: 08 E6 00 00
command: 5F 00 00 00
