Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 0A 00 00 00
#
name: CH
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 0C 00 00 00
#
name: TV/VCR
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 0D 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 0E 00 00 00
#
name: COUNTER_DISPLAY
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 10 00 00 00
#
name: F.FWD_>>_/_>>
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 11 00 00 00
#
name: REW_<<_/_<<
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 12 00 00 00
#
name: -REC/QTR-
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 14 00 00 00
#
name: PLAY_>
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 15 00 00 00
#
name: PAUSE/STILL
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 17 00 00 00
#
name: STOP_[]
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 1A 00 00 00
#
name: T-REC
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 1E 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 1F 00 00 00
#
name: CHANNEL_UP_^
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 40 00 00 00
#
name: CHANNEL_DOWN_V
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 41 00 00 00
#
name: TRACKING_+
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 46 00 00 00
#
name: TRACKING_-
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 47 00 00 00
#
name: EJECT
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 48 00 00 00
#
name: COUNTER_RESET
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 4C 00 00 00
#
name: INDEX_SEARCH
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 4D 00 00 00
#
name: TAPE_SPEED
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 50 00 00 00
#
name: COUNTER_MEMORY
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 51 00 00 00
#
name: COUNTER_CLOCK
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 56 00 00 00
#
name: A-TR
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 5C 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 81 00 00 00
#
name: CURSOR_>
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 83 00 00 00
#
name: CURSOR_<
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 84 00 00 00
#
name: VARIABLE_SEARCH_>>
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 85 00 00 00
#
name: VARIABLE_SEARCH_<<
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 86 00 00 00
#
name: INDEX_MARK
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 87 00 00 00
#
name: INDEX_ERASE
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 88 00 00 00
#
name: CURSOR_^
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 8D 00 00 00
#
name: CURSOR_V
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 8E 00 00 00
#
name: SUMMER_TIME
type: parsed
protocol: NECext
address: 7F 00 00 00
command: 90 00 00 00
