Filetype: IR signals file
Version: 1
#
name: FMMode
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 00 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 02 00 00 00
#
name: Reset
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 03 00 00 00
#
name: Test
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 05 00 00 00
#
name: DolbyDigital
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 06 00 00 00
#
name: Bypass
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 07 00 00 00
#
name: KEY_DVD
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 08 00 00 00
#
name: KEY_CD
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 09 00 00 00
#
name: Delay
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0A 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0D 00 00 00
#
name: Config
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0F 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 10 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 11 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 12 00 00 00
#
name: KEY_SLEEP
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 14 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 15 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 17 00 00 00
#
name: DSPDown
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 18 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 19 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1B 00 00 00
#
name: Opt
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1D 00 00 00
#
name: ChLevel
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1E 00 00 00
#
name: Coax
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1F 00 00 00
#
name: X_KEY_3Stereo
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 40 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 41 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 42 00 00 00
#
name: Dimmer
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 43 00 00 00
#
name: DTS
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 44 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 45 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 46 00 00 00
#
name: ProLogic
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 47 00 00 00
#
name: KEY_VCR
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 48 00 00 00
#
name: KEY_TAPE
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 49 00 00 00
#
name: KEY_AUX
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4A 00 00 00
#
name: Direct
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 50 00 00 00
#
name: PreTun
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 53 00 00 00
#
name: Memo
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 55 00 00 00
#
name: Auto
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 56 00 00 00
#
name: FMAM
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 57 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 59 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5E 00 00 00
#
name: DSPUp
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5F 00 00 00
