Filetype: IR signals file
Version: 1
#
name: VOLUME_-
type: parsed
protocol: NECext
address: 33 AA 00 00
command: 00 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 33 AA 00 00
command: 04 00 00 00
#
name: PLAY/PAUSE
type: parsed
protocol: NECext
address: 33 AA 00 00
command: 08 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 33 AA 00 00
command: 0C 00 00 00
#
name: VOLUME_+
type: parsed
protocol: NECext
address: 33 AA 00 00
command: 17 00 00 00
