Filetype: IR signals file
Version: 1
#
name: KEY_1
type: parsed
protocol: NECext
address: 11 00 00 00
command: 00 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 11 00 00 00
command: 01 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 11 00 00 00
command: 02 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 11 00 00 00
command: 03 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 11 00 00 00
command: 04 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 11 00 00 00
command: 05 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 11 00 00 00
command: 06 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 11 00 00 00
command: 07 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 11 00 00 00
command: 08 00 00 00
#
name: KEY_0
type: parsed
protocol: NECext
address: 11 00 00 00
command: 20 00 00 00
#
name: KEY_10CHANNELSUP
type: parsed
protocol: NECext
address: 11 00 00 00
command: 27 00 00 00
#
name: KEY_AGAIN
type: parsed
protocol: NECext
address: 11 00 00 00
command: 2C 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 11 00 00 00
command: 30 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 11 00 00 00
command: 31 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 11 00 00 00
command: 32 00 00 00
#
name: shuffle
type: parsed
protocol: NECext
address: 11 00 00 00
command: 35 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 11 00 00 00
command: 38 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 11 00 00 00
command: 39 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 11 00 00 00
command: 3A 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: 11 00 00 00
command: 3B 00 00 00
