Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 00 45 00 00
command: 80 00 00 00
#
name: VOLUME_+
type: parsed
protocol: NECext
address: 00 45 00 00
command: 85 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 00 45 00 00
command: 86 00 00 00
#
name: VOLUME_-
type: parsed
protocol: NECext
address: 00 45 00 00
command: 87 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 45 00 00
command: C4 00 00 00
