Filetype: IR signals file
Version: 1
# 
# America Lighting LEDs
# 
name: On
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 03 FC 00 00
#
name: Off
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 02 FD 00 00
#
name: White
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 04 FB 00 00
#
name: R_W_B
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 05 FA 00 00
#
name: Halloween
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 8981 4163 177 127 595 531 591 534 588 537 596 529 593 532 590 535 587 537 596 529 593 1659 596 1656 589 1664 591 1661 594 531 591 1661 594 1658 597 1655 590 1663 592 534 588 536 597 1655 590 536 597 528 594 531 591 533 589 535 587 1665 590 1662 593 532 590 1662 593 1658 597 1656 589 1664 591 40721 8965 2235 592
#
name: Xmas
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0A F5 00 00
#
name: Fade
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 13 EC 00 00
#
name: Quick
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0F F0 00 00
#
name: Pick_Color
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 08 F7 00 00
#
name: 3_Colors
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0C F3 00 00
#
name: 7_Colors
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 10 EF 00 00
#
name: 16_Colors
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 14 EB 00 00
#
name: Chase_Rt
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0E F1 00 00
#
name: Chase_Lt
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0D F2 00 00
#
name: Single_Rt
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 12 ED 00 00
#
name: Single_Lt
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 11 EE 00 00
#
name: Random
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 17 E8 00 00