Filetype: IR signals file
Version: 1
# 
name: PowerToggle
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0C 00 00 00
# 
name: VolumeUp
type: parsed
protocol: NEC
address: 20 00 00 00
command: 02 00 00 00
# 
name: VolumeDown
type: parsed
protocol: NEC
address: 20 00 00 00
command: 05 00 00 00
# 
name: VolumeMute
type: parsed
protocol: NEC
address: 20 00 00 00
command: 08 00 00 00
# 
name: ChannelUp
type: parsed
protocol: NEC
address: 20 00 00 00
command: 09 00 00 00
# 
name: ChannelDown
type: parsed
protocol: NEC
address: 20 00 00 00
command: 06 00 00 00
# 
name: FM
type: parsed
protocol: NEC
address: 20 00 00 00
command: 16 00 00 00
# 
name: BassUp
type: parsed
protocol: NEC
address: 20 00 00 00
command: 01 00 00 00
# 
name: BassDown
type: parsed
protocol: NEC
address: 20 00 00 00
command: 04 00 00 00
# 
name: InputAux
type: parsed
protocol: NEC
address: 20 00 00 00
command: 17 00 00 00
# 
name: InputBT
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0F 00 00 00
# 
name: InputLine
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0A 00 00 00
# 
name: Movie
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0B 00 00 00
# 
name: Music
type: parsed
protocol: NEC
address: 20 00 00 00
command: 10 00 00 00
# 
name: Scan
type: parsed
protocol: NEC
address: 20 00 00 00
command: 07 00 00 00
# 
name: TrebleUp
type: parsed
protocol: NEC
address: 20 00 00 00
command: 00 00 00 00
# 
name: TrebleDown
type: parsed
protocol: NEC
address: 20 00 00 00
command: 03 00 00 00
# 
name: Voice
type: parsed
protocol: NEC
address: 20 00 00 00
command: 14 00 00 00
