Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: B7 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: B7 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: B7 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: B7 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: B7 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: B7 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: B7 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: B7 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: B7 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: B7 00 00 00
command: 09 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 0B 00 00 00
#
name: CH_UP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 10 00 00 00
#
name: CH_DOWN
type: parsed
protocol: NECext
address: B7 00 00 00
command: 11 00 00 00
#
name: PWR_ON
type: parsed
protocol: NECext
address: B7 00 00 00
command: 2E 00 00 00
#
name: PWR_OFF
type: parsed
protocol: NECext
address: B7 00 00 00
command: 2F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: B7 00 00 00
command: 38 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: B7 00 00 00
command: 3A 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: B7 00 00 00
command: 63 00 00 00
#
name: TV/_DSS
type: parsed
protocol: NECext
address: B7 00 00 00
command: 69 00 00 00
#
name: JUMP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6C 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6E 00 00 00
#
name: FAVORITE
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6F 00 00 00
#
name: CURSER_UP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 72 00 00 00
#
name: CURSER_DOWN
type: parsed
protocol: NECext
address: B7 00 00 00
command: 73 00 00 00
#
name: CURSER_RIGHT
type: parsed
protocol: NECext
address: B7 00 00 00
command: 74 00 00 00
#
name: CURSER_LEFT
type: parsed
protocol: NECext
address: B7 00 00 00
command: 75 00 00 00
#
name: *
type: parsed
protocol: NECext
address: B7 00 00 00
command: 76 00 00 00
