Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 06 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 06 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 06 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 06 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 06 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 06 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 06 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 06 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 06 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 06 00 00 00
command: 09 00 00 00
#
name: sleep
type: parsed
protocol: NECext
address: 06 00 00 00
command: 0B 00 00 00
#
name: channel_up
type: parsed
protocol: NECext
address: 06 00 00 00
command: 10 00 00 00
#
name: channel_next
type: parsed
protocol: NECext
address: 06 00 00 00
command: 10 00 00 00
#
name: channel_down
type: parsed
protocol: NECext
address: 06 00 00 00
command: 11 00 00 00
#
name: channel_prev
type: parsed
protocol: NECext
address: 06 00 00 00
command: 11 00 00 00
#
name: vol_down
type: parsed
protocol: NECext
address: 06 00 00 00
command: 12 00 00 00
#
name: vol_up
type: parsed
protocol: NECext
address: 06 00 00 00
command: 13 00 00 00
#
name: video
type: parsed
protocol: NECext
address: 06 00 00 00
command: 14 00 00 00
#
name: audio
type: parsed
protocol: NECext
address: 06 00 00 00
command: 15 00 00 00
#
name: fav_main
type: parsed
protocol: NECext
address: 06 00 00 00
command: 16 00 00 00
#
name: mute
type: parsed
protocol: NECext
address: 06 00 00 00
command: 17 00 00 00
#
name: power
type: parsed
protocol: NECext
address: 06 00 00 00
command: 18 00 00 00
#
name: store
type: parsed
protocol: NECext
address: 06 00 00 00
command: 19 00 00 00
#
name: ext
type: parsed
protocol: NECext
address: 06 00 00 00
command: 1A 00 00 00
#
name: sys
type: parsed
protocol: NECext
address: 06 00 00 00
command: 1E 00 00 00
