Filetype: IR signals file
Version: 1
#
# BenQ DLP Projector W1070
# 
name: On
type: parsed
protocol: NECext
address: 00 30 00 00
command: 4F B0 00 00
# 
name: Off
type: parsed
protocol: NECext
address: 00 30 00 00
command: 4E B1 00 00
# 
name: HDMI_1
type: parsed
protocol: NECext
address: 00 30 00 00
command: 58 A7 00 00
# 
name: HDMI_2
type: parsed
protocol: NECext
address: 00 30 00 00
command: 59 A6 00 00
# 
name: Wireless
type: parsed
protocol: NECext
address: 00 30 00 00
command: 86 79 00 00
# 
name: Video
type: parsed
protocol: NECext
address: 00 30 00 00
command: 52 AD 00 00
# 
name: PC
type: parsed
protocol: NECext
address: 00 30 00 00
command: 41 BE 00 00
# 
name: Comp
type: parsed
protocol: NECext
address: 00 30 00 00
command: 51 AE 00 00
# 
name: Menu_Exit
type: parsed
protocol: NECext
address: 00 30 00 00
command: 0F F0 00 00
# 
name: EcoBlank
type: parsed
protocol: NECext
address: 00 30 00 00
command: 07 F8 00 00
# 
name: Auto
type: parsed
protocol: NECext
address: 00 30 00 00
command: 08 F7 00 00
# 
name: Source
type: parsed
protocol: NECext
address: 00 30 00 00
command: 04 FB 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 00 30 00 00
command: 0B F4 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 00 30 00 00
command: 0C F3 00 00
# 
name: Left_VolDwn
type: parsed
protocol: NECext
address: 00 30 00 00
command: 0D F2 00 00
# 
name: Right_VolUp
type: parsed
protocol: NECext
address: 00 30 00 00
command: 0E F1 00 00
# 
name: Mode_Enter
type: parsed
protocol: NECext
address: 00 30 00 00
command: 10 EF 00 00
# 
name: Aspect
type: parsed
protocol: NECext
address: 00 30 00 00
command: 13 EC 00 00
# 
name: PIP
type: parsed
protocol: NECext
address: 00 30 00 00
command: 1B E4 00 00
# 
name: SRS
type: parsed
protocol: NECext
address: 00 30 00 00
command: 99 66 00 00
# 
name: User1
type: parsed
protocol: NECext
address: 00 30 00 00
command: 75 8A 00 00
# 
name: User2
type: parsed
protocol: NECext
address: 00 30 00 00
command: 76 89 00 00
# 
name: User3
type: parsed
protocol: NECext
address: 00 30 00 00
command: 77 88 00 00
# 
name: Contrast
type: parsed
protocol: NECext
address: 00 30 00 00
command: 11 EE 00 00
# 
name: Bright
type: parsed
protocol: NECext
address: 00 30 00 00
command: 16 E9 00 00
# 
name: Sharp
type: parsed
protocol: NECext
address: 00 30 00 00
command: 7E 81 00 00
# 
name: Color
type: parsed
protocol: NECext
address: 00 30 00 00
command: 79 86 00 00
# 
name: ColorTemp
type: parsed
protocol: NECext
address: 00 30 00 00
command: 5F A0 00 00
# 
name: Tint
type: parsed
protocol: NECext
address: 00 30 00 00
command: 7A 85 00 00
# 
name: Finetune
type: parsed
protocol: NECext
address: 00 30 00 00
command: 5D A2 00 00
# 
name: 3D
type: parsed
protocol: NECext
address: 00 30 00 00
command: 8D 72 00 00
# 
name: Invert
type: parsed
protocol: NECext
address: 00 30 00 00
command: 9D 62 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 00 30 00 00
command: 14 EB 00 00
# 
name: Freeze
type: parsed
protocol: NECext
address: 00 30 00 00
command: 03 FC 00 00
# 
name: Test
type: parsed
protocol: NECext
address: 00 30 00 00
command: 94 6B 00 00
