Filetype: IR signals file
Version: 1
#
name: SELECT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 11 00 00 00
#
name: MULTISCREEN_SELECT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 11 00 00 00
#
name: DIGITAL_2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 17 00 00 00
#
name: VIDEO_5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1B 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 7D 00 00 00
