Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 09 00 00 00
#
name: KEY_102ND
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0A 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0C 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0D 00 00 00
#
name: KEY_HELP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 11 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 20 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 21 00 00 00
#
name: KEY_REDO
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 22 00 00 00
#
name: KEY_AB
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 23 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 29 00 00 00
#
name: KEY_CANCEL
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2F 00 00 00
#
name: KEY_EXIT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 38 00 00 00
#
name: KEY_TEXT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 3C 00 00 00
#
name: KEY_EPG
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 4F 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 52 00 00 00
#
name: KEY_RADIO
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 53 00 00 00
#
name: KEY_SELECT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 57 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6B 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6C 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6D 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6E 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 76 00 00 00
