Filetype: IR signals file
Version: 1
#
name: MD
type: parsed
protocol: NECext
address: 17 00 00 00
command: 3F 00 00 00
#
name: TAPE_2
type: parsed
protocol: NECext
address: 17 00 00 00
command: 3F 00 00 00
#
name: DCC
type: parsed
protocol: NECext
address: 17 00 00 00
command: 3F 00 00 00
#
name: INPUT_-_MD
type: parsed
protocol: NECext
address: 17 00 00 00
command: 3F 00 00 00
