Filetype: IR signals file
Version: 1
#
name: FRAME_>>
type: parsed
protocol: NECext
address: B4 00 00 00
command: 2A 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: B4 00 00 00
command: 2A 00 00 00
#
name: 
type: parsed
protocol: NECext
address: B4 00 00 00
command: 2A 00 00 00
#
name: FRAME_<<
type: parsed
protocol: NECext
address: B4 00 00 00
command: 2B 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: B4 00 00 00
command: 2B 00 00 00
#
name: VIDEO_1
type: parsed
protocol: NECext
address: B4 00 00 00
command: 35 00 00 00
#
name: INPUT_1_VTR_1
type: parsed
protocol: NECext
address: B4 00 00 00
command: 35 00 00 00
#
name: VIDEO_2
type: parsed
protocol: NECext
address: B4 00 00 00
command: 36 00 00 00
#
name: VIDEO_3
type: parsed
protocol: NECext
address: B4 00 00 00
command: 37 00 00 00
#
name: VIDEO_4
type: parsed
protocol: NECext
address: B4 00 00 00
command: 38 00 00 00
#
name: VIDEO_5
type: parsed
protocol: NECext
address: B4 00 00 00
command: 3C 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: B4 00 00 00
command: 43 00 00 00
#
name: VCR_PLUS
type: parsed
protocol: NECext
address: B4 00 00 00
command: 60 00 00 00
#
name: VCR_PLUS+
type: parsed
protocol: NECext
address: B4 00 00 00
command: 60 00 00 00
#
name: VCR_PLUS:_ONCE
type: parsed
protocol: NECext
address: B4 00 00 00
command: 61 00 00 00
#
name: SET
type: parsed
protocol: NECext
address: B4 00 00 00
command: 61 00 00 00
#
name: VCR_PLUS:_DAILY
type: parsed
protocol: NECext
address: B4 00 00 00
command: 62 00 00 00
#
name: VCR_PLUS:_WEEKLY
type: parsed
protocol: NECext
address: B4 00 00 00
command: 63 00 00 00
