Filetype: IR signals file
Version: 1
#
name: KEY_0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: KEY_1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: KEY_2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: KEY_3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: KEY_4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: KEY_5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: KEY_6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: KEY_7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: KEY_8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: KEY_9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: KEY_P
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: KEY_LIST
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: KEY_MEDIA
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: KEY_S
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: KEY_CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: KEY_CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: KEY_DIGITS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 25 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: KEY_TIME
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: KEY_SAVE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: KEY_REDO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: KEY_PROPS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: KEY_MAX
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: KEY_YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: KEY_A
type: parsed
protocol: NECext
address: 00 00 00 00
command: 33 00 00 00
#
name: KEY_BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: KEY_SHOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: KEY_GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: KEY_RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: KEY_INSERT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3A 00 00 00
#
name: KEY_MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3B 00 00 00
#
name: KEY_TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: KEY_SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3E 00 00 00
