Filetype: IR signals file
Version: 1
#
name: KEY_POWER
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0C 00 00 00
#
name: KEY_PROG1
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0D 00 00 00
#
name: KEY_MUTE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0E 00 00 00
#
name: KEY_INFO
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0F 00 00 00
#
name: KEY_VOLUMEUP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 10 00 00 00
#
name: KEY_VOLUMEDOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 11 00 00 00
#
name: KEY_PAGEUP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 12 00 00 00
#
name: KEY_PAGEDOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 13 00 00 00
#
name: KEY_FASTFORWARD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 14 00 00 00
#
name: KEY_REWIND
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 15 00 00 00
#
name: KEY_PLAY
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 16 00 00 00
#
name: KEY_RECORD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 17 00 00 00
#
name: KEY_PAUSE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 18 00 00 00
#
name: KEY_STOP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 19 00 00 00
#
name: KEY_NEXT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1A 00 00 00
#
name: KEY_PREVIOUS
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1B 00 00 00
#
name: KEY_UP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1E 00 00 00
#
name: KEY_DOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1F 00 00 00
#
name: KEY_LEFT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 20 00 00 00
#
name: KEY_RIGHT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 21 00 00 00
#
name: KEY_OK
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 22 00 00 00
#
name: KEY_BACK
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 23 00 00 00
#
name: KEY_DVD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 24 00 00 00
#
name: KEY_VCR
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 25 00 00 00
#
name: KEY_LIST
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 26 00 00 00
#
name: KEY_LIST
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 26 00 00 00
#
name: KEY_TV
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 48 00 00 00
