Filetype: IR signals file
Version: 1
# 
# Hitachi RC43140 TV
# 
# Likely works for 32HE2000 55HK6000 65HL8000 55HL7000 32HE4000 24HE2000 49HK6500 43HK6500 55HK6500
# 43HL8000 49HL8000 55HL8000K 43HL8000K 43HE4000 40HE4001 49HE4000 40HE4000 32HE4500 43HK6000
# 43HK6001 32HE4500K 55HL8000 24HE2001 65HL7000 43F501HK6000 55HL9000G 49HL7000 49HK6000
# 
name: POWER
type: parsed
protocol: RC5
address: 03 00 00 00
command: 0C 00 00 00
# 
name: VOL+
type: parsed
protocol: RC5
address: 03 00 00 00
command: 10 00 00 00
# 
name: VOL-
type: parsed
protocol: RC5
address: 03 00 00 00
command: 11 00 00 00
# 
name: CH+
type: parsed
protocol: RC5
address: 03 00 00 00
command: 20 00 00 00
# 
name: CH-
type: parsed
protocol: RC5
address: 03 00 00 00
command: 21 00 00 00
# 
name: MUTE
type: parsed
protocol: RC5
address: 03 00 00 00
command: 0D 00 00 00
# 
name: Input
type: parsed
protocol: RC5
address: 03 00 00 00
command: 38 00 00 00
# 
name: Home
type: parsed
protocol: RC5
address: 03 00 00 00
command: 30 00 00 00
# 
name: Lang
type: parsed
protocol: RC5
address: 03 00 00 00
command: 0F 00 00 00
# 
name: Txt
type: parsed
protocol: RC5
address: 03 00 00 00
command: 3C 00 00 00
# 
name: Info
type: parsed
protocol: RC5
address: 03 00 00 00
command: 12 00 00 00
# 
name: G
type: parsed
protocol: RC5
address: 03 00 00 00
command: 2F 00 00 00
# 
name: Up
type: parsed
protocol: RC5
address: 03 00 00 00
command: 14 00 00 00
# 
name: Down
type: parsed
protocol: RC5
address: 03 00 00 00
command: 13 00 00 00
# 
name: Left
type: parsed
protocol: RC5
address: 03 00 00 00
command: 15 00 00 00
# 
name: Right
type: parsed
protocol: RC5
address: 03 00 00 00
command: 16 00 00 00
# 
name: Ok
type: parsed
protocol: RC5
address: 03 00 00 00
command: 35 00 00 00
# 
name: Back
type: parsed
protocol: RC5
address: 03 00 00 00
command: 0A 00 00 00
# 
name: Exit
type: parsed
protocol: RC5
address: 03 00 00 00
command: 25 00 00 00
# 
name: Netflix
type: parsed
protocol: RC5
address: 03 00 00 00
command: 27 00 00 00
# 
name: Youtube
type: parsed
protocol: RC5
address: 03 00 00 00
command: 29 00 00 00
# 
name: Favorite
type: parsed
protocol: RC5
address: 03 00 00 00
command: 3B 00 00 00
# 
name: Prime
type: parsed
protocol: RC5
address: 03 00 00 00
command: 3E 00 00 00
# 
name: Red
type: parsed
protocol: RC5
address: 03 00 00 00
command: 37 00 00 00
# 
name: Green
type: parsed
protocol: RC5
address: 03 00 00 00
command: 36 00 00 00
# 
name: Yellow
type: parsed
protocol: RC5
address: 03 00 00 00
command: 32 00 00 00
# 
name: Blue
type: parsed
protocol: RC5
address: 03 00 00 00
command: 34 00 00 00
# 
name: Rew
type: parsed
protocol: RC5
address: 03 00 00 00
command: 1B 00 00 00
# 
name: Pause
type: parsed
protocol: RC5
address: 03 00 00 00
command: 31 00 00 00
# 
name: Fwd
type: parsed
protocol: RC5
address: 03 00 00 00
command: 1C 00 00 00
# 
name: Rec
type: parsed
protocol: RC5
address: 03 00 00 00
command: 33 00 00 00
# 
name: Play
type: parsed
protocol: RC5
address: 03 00 00 00
command: 19 00 00 00
# 
name: Stop
type: parsed
protocol: RC5
address: 03 00 00 00
command: 18 00 00 00
# 
name: 1
type: parsed
protocol: RC5
address: 03 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: RC5
address: 03 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: RC5
address: 03 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: RC5
address: 03 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: RC5
address: 03 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: RC5
address: 03 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: RC5
address: 03 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: RC5
address: 03 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: RC5
address: 03 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: RC5
address: 03 00 00 00
command: 00 00 00 00
