Filetype: IR signals file
Version: 1
# 
# Teufel 3SIXTY Speakers
#
name: POWER
type: parsed
protocol: NEC
address: FD 00 00 00
command: E2 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: FD 00 00 00
command: E1 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: FD 00 00 00
command: E7 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: FD 00 00 00
command: B9 00 00 00
# 
name: Reverse
type: parsed
protocol: NEC
address: FD 00 00 00
command: BA 00 00 00
# 
name: Forward
type: parsed
protocol: NEC
address: FD 00 00 00
command: EA 00 00 00
# 
name: Play Pause
type: parsed
protocol: NEC
address: FD 00 00 00
command: BD 00 00 00
# 
name: Input
type: parsed
protocol: NEC
address: FD 00 00 00
command: FC 00 00 00
# 
name: Link
type: parsed
protocol: NEC
address: FD 00 00 00
command: FD 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: FD 00 00 00
command: AE 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: FD 00 00 00
command: FB 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: FD 00 00 00
command: BB 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: FD 00 00 00
command: EB 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: FD 00 00 00
command: AB 00 00 00
# 
name: Favorite
type: parsed
protocol: NEC
address: FD 00 00 00
command: ED 00 00 00
