Filetype: IR signals file
Version: 1
# 
name: Standby
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: 04 00 00 00
command: 45 00 00 00
# 
name: OpenClose
type: parsed
protocol: NEC
address: 04 00 00 00
command: 17 00 00 00
# 
name: Repeat
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 04 00 00 00
command: 14 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0D 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1B 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 04 00 00 00
command: 49 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 04 00 00 00
command: 11 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 04 00 00 00
command: 19 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1E 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 04 00 00 00
command: 01 00 00 00
# 
name: 10
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0F 00 00 00
# 
name: Speaker
type: parsed
protocol: NEC
address: 04 00 00 00
command: 00 00 00 00
# 
name: Treb_min
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5B 00 00 00
# 
name: Treb_plus
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4F 00 00 00
# 
name: A_B
type: parsed
protocol: NEC
address: 04 00 00 00
command: 15 00 00 00
# 
name: B_Ward
type: parsed
protocol: NEC
address: 04 00 00 00
command: 58 00 00 00
# 
name: Stop
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4B 00 00 00
# 
name: F_Ward
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4C 00 00 00
# 
name: USB
type: parsed
protocol: NEC
address: 04 00 00 00
command: 18 00 00 00
# 
name: Bass_min
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1D 00 00 00
# 
name: Bass_plus
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Prev
type: parsed
protocol: NEC
address: 04 00 00 00
command: 04 00 00 00
# 
name: Vol_plus
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
# 
name: Next
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5E 00 00 00
# 
name: Vol_min
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
# 
name: Input
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0A 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
