Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 00 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 02 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 04 00 00 00
#
name: NUMERIC_STAR
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 06 00 00 00
#
name: OPTION
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 07 00 00 00
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 09 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 0B 00 00 00
#
name: HEART
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 0F 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 10 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 11 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 12 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 14 00 00 00
#
name: MAIL
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 15 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1C 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1E 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1F 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 20 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 21 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 22 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 23 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 24 00 00 00
#
name: X
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 25 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 27 00 00 00
#
name: NUMERIC_POUND
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 28 00 00 00
#
name: TV/AV
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 2A 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 2B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 2E 00 00 00
#
name: HOME
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 2F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 31 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 33 00 00 00
#
name: ?
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 37 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 3B 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 3E 00 00 00
