Filetype: IR signals file
Version: 1
#
name: VIDEO_2
type: parsed
protocol: NECext
address: 03 00 00 00
command: 12 00 00 00
#
name: VIDEO_3
type: parsed
protocol: NECext
address: 03 00 00 00
command: 14 00 00 00
#
name: TV_POWER
type: parsed
protocol: NECext
address: 03 00 00 00
command: 17 00 00 00
