Filetype: IR signals file
Version: 1
#
name: OK
type: parsed
protocol: NECext
address: 83 33 00 00
command: 41 00 00 00
#
name: DIRECTION_UP
type: parsed
protocol: NECext
address: 83 33 00 00
command: 42 00 00 00
#
name: DIRECTION_DOWN
type: parsed
protocol: NECext
address: 83 33 00 00
command: 43 00 00 00
#
name: DIRECTION_LEFT
type: parsed
protocol: NECext
address: 83 33 00 00
command: 44 00 00 00
#
name: DIRECTION_RIGHT
type: parsed
protocol: NECext
address: 83 33 00 00
command: 45 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 83 33 00 00
command: 46 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 83 33 00 00
command: 47 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 83 33 00 00
command: 48 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 83 33 00 00
command: 49 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 83 33 00 00
command: 50 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 83 33 00 00
command: 51 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 83 33 00 00
command: 52 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 83 33 00 00
command: 53 00 00 00
#
name: PICTURE_IN_PICTURE
type: parsed
protocol: NECext
address: 83 33 00 00
command: 54 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 83 33 00 00
command: 55 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 83 33 00 00
command: 56 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 83 33 00 00
command: 57 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 83 33 00 00
command: 58 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 83 33 00 00
command: 59 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 83 33 00 00
command: 60 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 83 33 00 00
command: 61 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 83 33 00 00
command: 62 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 83 33 00 00
command: 63 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 83 33 00 00
command: 64 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 83 33 00 00
command: 65 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 83 33 00 00
command: 66 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 83 33 00 00
command: 67 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 83 33 00 00
command: 68 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 83 33 00 00
command: 69 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 83 33 00 00
command: 70 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 83 33 00 00
command: 71 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 83 33 00 00
command: 72 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 83 33 00 00
command: 73 00 00 00
