Filetype: IR signals file
Version: 1
#
# LILUCO LED
# Autogenerated from ircodes/LILUCO/LED.xml
#
name: -
type: parsed
protocol: NECext
address: F7 00 00 00
command: 7F 80 00 00
#
name: +
type: parsed
protocol: NECext
address: F7 00 00 00
command: FF 00 00 00
#
name: OFF
type: parsed
protocol: NECext
address: F7 00 00 00
command: BF 40 00 00
#
name: POWER
type: parsed
protocol: NECext
address: F7 00 00 00
command: 3F C0 00 00
#
name: R
type: parsed
protocol: NECext
address: F7 00 00 00
command: DF 20 00 00
#
name: G
type: parsed
protocol: NECext
address: F7 00 00 00
command: 5F A0 00 00
#
name: B
type: parsed
protocol: NECext
address: F7 00 00 00
command: 9F 60 00 00
#
name: W
type: parsed
protocol: NECext
address: F7 00 00 00
command: 1F E0 00 00
#
name: R
type: parsed
protocol: NECext
address: F7 00 00 00
command: EF 10 00 00
#
name: G
type: parsed
protocol: NECext
address: F7 00 00 00
command: 6F 90 00 00
#
name: B
type: parsed
protocol: NECext
address: F7 00 00 00
command: AF 50 00 00
#
name: FLASH
type: parsed
protocol: NECext
address: F7 00 00 00
command: 2F D0 00 00
#
name: R
type: parsed
protocol: NECext
address: F7 00 00 00
command: CF 30 00 00
#
name: G
type: parsed
protocol: NECext
address: F7 00 00 00
command: 4F B0 00 00
#
name: B
type: parsed
protocol: NECext
address: F7 00 00 00
command: 8F 70 00 00
#
name: STROBE
type: parsed
protocol: NECext
address: F7 00 00 00
command: 0F F0 00 00
#
name: R
type: parsed
protocol: NECext
address: F7 00 00 00
command: F7 08 00 00
#
name: G
type: parsed
protocol: NECext
address: F7 00 00 00
command: 77 88 00 00
#
name: B
type: parsed
protocol: NECext
address: F7 00 00 00
command: B7 48 00 00
#
name: FADE
type: parsed
protocol: NECext
address: F7 00 00 00
command: 37 C8 00 00
#
name: R
type: parsed
protocol: NECext
address: F7 00 00 00
command: D7 28 00 00
#
name: G
type: parsed
protocol: NECext
address: F7 00 00 00
command: 57 A8 00 00
#
name: B
type: parsed
protocol: NECext
address: F7 00 00 00
command: 97 68 00 00
#
name: SMOOTH
type: parsed
protocol: NECext
address: F7 00 00 00
command: 17 E8 00 00
