Filetype: IR signals file
Version: 1
#
name: 2-3-5
type: parsed
protocol: NECext
address: BA 01 00 00
command: 00 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: BA 01 00 00
command: 01 00 00 00
#
name: VOLUME_DOWN
type: parsed
protocol: NECext
address: BA 01 00 00
command: 02 00 00 00
#
name: VOLUME_UP
type: parsed
protocol: NECext
address: BA 01 00 00
command: 03 00 00 00
#
name: FM/AM
type: parsed
protocol: NECext
address: BA 01 00 00
command: 06 00 00 00
#
name: SURROUND_-
type: parsed
protocol: NECext
address: BA 01 00 00
command: 0A 00 00 00
#
name: SURROUND_+
type: parsed
protocol: NECext
address: BA 01 00 00
command: 0B 00 00 00
#
name: VCR
type: parsed
protocol: NECext
address: BA 01 00 00
command: 0D 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: BA 01 00 00
command: 0E 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: BA 01 00 00
command: 0F 00 00 00
#
name: CHANNEL_DOWN
type: parsed
protocol: NECext
address: BA 01 00 00
command: 18 00 00 00
#
name: CHANNEL_UP
type: parsed
protocol: NECext
address: BA 01 00 00
command: 19 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: BA 01 00 00
command: 1A 00 00 00
#
name: ARROW_DOWN
type: parsed
protocol: NECext
address: BA 01 00 00
command: 20 00 00 00
#
name: TUNE_DOWN
type: parsed
protocol: NECext
address: BA 01 00 00
command: 20 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: BA 01 00 00
command: 40 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: BA 01 00 00
command: 41 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: BA 01 00 00
command: 42 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: BA 01 00 00
command: 43 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: BA 01 00 00
command: 44 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: BA 01 00 00
command: 45 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: BA 01 00 00
command: 46 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: BA 01 00 00
command: 47 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: BA 01 00 00
command: 48 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: BA 01 00 00
command: 49 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: BA 01 00 00
command: 4C 00 00 00
#
name: MUTE_ALL
type: parsed
protocol: NECext
address: BA 01 00 00
command: 4D 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: BA 01 00 00
command: 52 00 00 00
#
name: CD/DVD
type: parsed
protocol: NECext
address: BA 01 00 00
command: 53 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: BA 01 00 00
command: 55 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: BA 01 00 00
command: 56 00 00 00
#
name: <<
type: parsed
protocol: NECext
address: BA 01 00 00
command: 57 00 00 00
#
name: >>
type: parsed
protocol: NECext
address: BA 01 00 00
command: 58 00 00 00
#
name: SHUFFLE
type: parsed
protocol: NECext
address: BA 01 00 00
command: 5C 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: BA 01 00 00
command: 60 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: BA 01 00 00
command: 80 00 00 00
#
name: SETTINGS
type: parsed
protocol: NECext
address: BA 01 00 00
command: 80 00 00 00
#
name: DVD_MENU
type: parsed
protocol: NECext
address: BA 01 00 00
command: 90 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: BA 01 00 00
command: 9D 00 00 00
#
name: ARROW_LEFT
type: parsed
protocol: NECext
address: BA 01 00 00
command: A0 00 00 00
#
name: ARROW_UP
type: parsed
protocol: NECext
address: BA 01 00 00
command: C0 00 00 00
#
name: TUNE_UP
type: parsed
protocol: NECext
address: BA 01 00 00
command: C0 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: BA 01 00 00
command: D0 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: BA 01 00 00
command: E0 00 00 00
