Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 00 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 01 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 02 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 03 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 05 00 00 00
#
name: TopMenu
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 06 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 07 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 08 00 00 00
#
name: AngleReplay
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 09 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0A 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0B 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0C 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0D 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0E 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 0F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 19 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 1A 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 1C 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 1E 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 1F 00 00 00
#
name: PauseStep
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 20 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 21 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 22 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 23 00 00 00
#
name: Rev
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 26 00 00 00
#
name: FwdSlow
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 29 00 00 00
#
name: RevSlow
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 2C 00 00 00
#
name: LastMemo
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 2F 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 35 00 00 00
#
name: ABRepeat
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 36 00 00 00
#
name: SearchMode
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 38 00 00 00
#
name: ProgramRandom
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 39 00 00 00
#
name: PictureMode
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 3A 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 3B 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 3C C4 00 00
command: 4A 00 00 00
