Filetype: IR signals file
Version: 1
#
name: 7
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 00 00 00 00
#
name: C
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 02 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 03 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 05 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 06 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 08 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 09 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 0A 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 0C 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 0D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 0E 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 10 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 11 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 15 00 00 00
#
name: RWD
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 16 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 20 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 21 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 22 00 00 00
#
name: SEARCH_MODE
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 23 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 29 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2A 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2B 00 00 00
#
name: RRWD
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2C 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 2F 00 00 00
#
name: A_B
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 30 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 32 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 34 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 34 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 36 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 37 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 38 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 3C 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 1D 00 00 00
command: 3F 00 00 00
